================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
该样例演示了序列扫描采样，扫描全部通道，旋转开发板上的滑动电阻器R11调节Chanel0输入电压，
旋转开发板上的滑动电阻器R24调节Chanel1输入电压，串口实时打印数据，，LED1每隔1s翻转一次。

Function description:
This example demonstrates sequence scanning sampling, scanning all channels, 
rotating the sliding resistor R11 on the development board to adjust the input 
voltage of Chanel0, Rotate the sliding resistor R24 on the development board to 
adjust the input voltage of Chanel1, and print data in real-time through the 
serial port,, LED1 flips every 1 second.
================================================================================
测试环境：
测试用板：DPM32M08X_EVB V1.0
MDK版本： 5.38


Test environment:
Test board: DPM32M08X_EVB V1.0
MDK Version: 5.38

================================================================================
使用步骤：
1. 接上P2上的PA0跳线帽，将PA0接到滑动变阻器，接上P10上的跳线帽，将串口接到USB。
2. 编译下载程序到MCU，并运行。
3. 可观察到开发板上的LED1每隔1s翻转一次。
4. 旋转的滑动变阻器R11，R24，串口实时输出采样电压。

Example execution steps:
1. Connect the PA0 jumper cap on P2, connect PA0 to the sliding resistor, connect the jumper cap on P10, and connect the serial port to USB.
2. Compile and download the program to MCU, and run it.
3. It can be observed that LED1 on the development board flips every 1 second.
4. Rotating sliding rheostat R11, R24， Real time output of sampling voltage through serial port.
================================================================================
注意事项：
LED引脚如下：
LED1       -> PC10

ADC引脚如下：
ADC_CH0    -> PA0
ADC_CH1    -> PA1

UART引脚如下：
UART_Tx    -> PA9
UART_Rx    -> PA10

Notes:
The LED pins are as follows:
LED1       -> PC10

The ADC pins are as follows:
ADC_CH0    -> PA0
ADC_CH1    -> PA1

The UART pins are as follows:
UART_Tx    -> PA9
UART_Rx    -> PA10
================================================================================