================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
该样例演示了ADC通道插队采样功能，通道1-13序列采样，通道0插队采样，触发插队后，从插队
结果寄存器读取采样值，旋转开发板上的滑动电阻器R11调节输入电压，串口实时打印采样数据，
LED1每隔1s翻转一次。

Function descriptions:
This example demonstrates the ADC channel queueing sampling function, with 
sequence sampling from channels 1-13 and queueing sampling from channel 0. 
After triggering queueing, the queueing process starts from The result register 
reads the sampling value, rotates the sliding resistor R11 on the development 
board to adjust the input voltage, and the serial port prints the sampling data 
in real time, LED1 flips every 1 second.
================================================================================
测试环境：
测试用板：DPM32M08X_EVB V1.0
MDK版本： 5.38


Test environment:
Test board: DPM32M08X_EVB V1.0
MDK Version: 5.38

================================================================================
使用步骤：
1. 接上P2上的PA0跳线帽，将PA0接到滑动变阻器，接上P10上的跳线帽，将串口接到USB。
2. 编译下载程序到MCU，并运行。
3. 可观察到开发板上的LED1每隔1s翻转一次。
4. 旋转的滑动变阻器R11，串口实时输出插队采样电压。

Example execution steps:
1. Connect the PA0 jumper cap on P2 and connect PA0 to the sliding rheostat, connect
 the jumper cap on P10, and connect the serial port to USB.
2. Compile and download the program to MCU, and run it.
3. It can be observed that LED1 on the development board flips every 1 second.
4. The rotating sliding rheostat R11 outputs real-time queue sampling voltage 
through the serial port.
================================================================================
注意事项：
LED引脚如下：
LED1       -> PC10

ADC引脚如下：
ADC_CH0    -> PA0

UART引脚如下：
UART_Tx    -> PA9
UART_Rx    -> PA10

Notes:
The LED pins are as follows:
LED1       -> PC10

The ADC pins are as follows:
ADC_CH0    -> PA0

The UART pins are as follows:
UART_Tx    -> PA9
UART_Rx    -> PA10
================================================================================